**Manufacturer: Jacksons Fencing**

**Web: www.jacksons-security.co.uk**

**Tel: +44 (0)1233 750393 | 0800 953 3699**

**Product Reference: JAKSUN® SOLAR FENCE PANEL**

Solar fence panel system for vertical installation in ground

**Guarantee:**

Timber components covered by our 25 year Jakcure guarantee against rot and insect attack

Solar panel covered by 25 year product warranty and 25 year linear power output warranty provided by the solar panel manufacturer

**Solar Fence Panel Output:**

Electrical Peak power - 425W

Vmpp - 32.96V

Voc - 39.23V

Impp - 12.90A

Isc - 13.93A

**Fencing & Posts:**

Solar fence panel - 1170mm High, 1830mm Wide, 50mm Thick

600mm High Venetian Hit and Miss timber fence panel underneath [delete if not required]

*We recommend installing Jaksun solar fence panels on top of 600mm high timber fence panels. With the required gravel board and capping the total fence height is just under two metres.*

**Gravel board:**

Jakcure pressure treated gravel board 140mm high.

Jakcure pressure treated hedgehog friendly gravel board 140mm high.

*A gravel board must be used to comply with guarantee terms and conditions, where panel is in contact with the ground.*

**Posts:**

Slotted Jakposts adapted for solar panel cables, dependent on fence height (panel combination)

**Fixings:**

Stainless steel panel screws

**Finish / Colour:**

Jakcure® treated timber as standard

Planed timber finish

**Installation**

In accordance with manufacturer’s instructions

**NOTES:**

For more information please contact Jacksons Fencing. We reserve the right to alter specification within this document at any time.