**Urban Panel**

Manufacturer: Jacksons Fencing.

Web: [www.jacksons-fencing.co.uk](javascript:NavigateToWebsite('www.jacksons-fencing.co.uk',%20'09474',%20'JacksonsFencing__',%20false);).

Tel: +44 (0)1233 750393.

**Product reference:**

Urban Panel

**Width – As Standard:**

1.83m

**Height:**

1.83m

Thickness: 51mm

Framing: 45 x 51mm section planed.

Pales: 95 x 8mm thickness & 38 x 7mm. Planed

**Gravel Boards:**

Gravel boards are required where panels are in contact with the ground. 140mm added to the height.

**Posts:**

Slotted Jakposts®

**Guarantee:**

All timber used throughout is superior quality Jakcure® treated softwood guaranteed for 25 years.

**Features:**

* All fixings are stainless steel.
* Gravel boards are required where panels are in contact with the ground.
* Morticed and tenoned frame for extra strength.
* Part of our ‘good-both-sides’ range.
* Panels can be rotated so the pales can run either vertically or horizontally.

**Gates:**

Gates are Jakcure® treated softwood, right and left hand hanging (when viewed from the outside) but are made to order. They are designed to match our Urban Panel.

Height: 1.93m (plus capping).

Width: 1m

**Installation**

In accordance to manufacturer’s instructions.

Combining wide and narrow timber pales, Urban is a contemporary panel with a distinctive design, ideal for a variety of applications. Mortice and tennoned frame for extra strength, these panels are planed all round for a smooth finish, with stainless steel fixings throughout to ensure a long life.

For additional information, please contact Jacksons Fencing. All information within was correct at time of creation. We reserve the right to alter specification without notice.