**Canterbury Combi Panel**

Manufacturer: Jacksons Fencing.

Web: [www.jacksons-fencing.co.uk](javascript:NavigateToWebsite('www.jacksons-fencing.co.uk',%20'09474',%20'JacksonsFencing__',%20false);).

Tel: +44 (0)1233 750393.

**Product reference:**

Canterbury Combi Panel

**Width – As Standard:**

1.83m

**Height:**

1.83m

Panel is frameless for a contemporary look.

Panel Thickness: 51mm

Venetian slats: 45 x 16mm

**Gravel Boards:**

Gravel boards are required where panels are in contact with the ground. 140mm added to the height.

**Posts:**

Slotted Jakposts®

**Guarantee:**

All timber used throughout is superior quality Jakcure® treated softwood guaranteed for 25 years.

**Features:**

* All fixings are stainless steel.
* Gravel boards are required where panels are in contact with the ground.
* Panel is frameless for a contemporary design.
* All timber is planed all round.

**Gates:**

Canterbury Combi boarded gates are both robust and versatile that will give privacy to any property while complementing the Canterbury Combi panel. Supplied in natural Jakcure® treated finish, right and left hand hanging (when viewed from the outside).

Height: 1.93m

Width: 1m

**Installation**

In accordance to manufacturer’s instructions.

These premium contemporary panels combine two of Jacksons’ most popular products: horizontal Tongue and Groove with our ever-popular Venetian. Canterbury Combi lends a sleek, modern and linear look to any garden, with the added benefits of privacy and protection from the wind.

For additional information, please contact Jacksons Fencing. All information within was correct at time of creation. We reserve the right to alter specification without notice.