**Chilham Panel**

Manufacturer: Jacksons Fencing.

Web: [www.jacksons-fencing.co.uk](javascript:NavigateToWebsite('www.jacksons-fencing.co.uk',%20'09474',%20'JacksonsFencing__',%20false);).

Tel: +44 (0)1233 750393.

**Product reference:**

Chilham Panel

**Width – As Standard:**

1.83m

**Height:**

0.91m

1.22m

1.52m

1.65m

Framing: Top/bottom - 45 x 70mm planed. Sides 45 x 51mm planed.

Panel Thickness: 51mm Infill panels: 95 x 8mm.

Assembly system with vertical pales that overlap/interlock with the infill panels.

**Gravel Boards:**

Gravel boards are required where panels are in contact with the ground. 140mm added to the height.

**Posts:**

Slotted Jakposts®

**Guarantee:**

All timber used throughout is superior quality Jakcure® treated softwood guaranteed for 25 years.

**Features:**

* All fixings are stainless steel.
* Gravel boards are required where panels are in contact with the ground.
* Has a unique interlocking grooved board system.
* Part of our premium ‘good-both-sides’ range.

**Gates:**

Gates are Jakcure® treated softwood, right and left hand hanging (when viewed from the outside) as standard, designed to match our Chilham Panel.

Height: 1.78m (plus capping).

Width: 1m

**Installation**

In accordance to manufacturer’s instructions.

It’s a challenge to design a solid timber fence that looks equally good on both sides. However, our Chilham panels manage just that, in a unique design, free from horizontal rails that could spoil either yours or your neighbour’s view.

For additional information, please contact Jacksons Fencing. All information within was correct at time of creation. We reserve the right to alter specification without notice.